请将当前目录所有文件复制到电脑硬盘，然后运行文件夹内的RFIDCalibration.exe

使用说明：
1、点击“刷新”按钮，检查当前连接的打印机信息是否正确；
2、设置读功率：12，写功率：15，校准模式：2，工作频率（Auto），点击“更改设置”按钮；
3、安装好RFID标签和碳带后，点击“开始校准”按钮，此时打印机将开始出纸；
4、待打印机出纸停止后，将显示校准结果；
5、标签纸校准曲线下方的图片，是标签定位波形图；
6、RFID信号范围图示下方的图片，是单张RFID标签的信号分布图示。

系统要求：
WinXP,Win7,Win8.1,Win10,Win11
WinXP要求已安装.NET Framework 2.0以上版本

注意：
WinXP操作系统默认没有安装.net，请搜索下载并安装.Net Framework 2.0后运行RFIDCalibration.exe.

技术支持：
工作日9点30分到17点30分
电话号码：0755-23213336
其它时间请访问我们的网站获取更多的技术支持信息或者发送电子邮件地址到: support@zmin.com.cn

深圳致明兴科技有限公司
http://www.zmin.com.cn


RFIDCalibration tool instructions: 

Please run "RFIDCalibration.exe".

1. Click the "Refresh" button to check if the currently connected printer information is correct.
2, Set the Read power (factory default 12), Write power (factory default 15), calibration mode (2 is recommended), click the "setting" button;
3. After installing the RFID tag and ribbon, click the “Start Calibration” button, and the printer will start to output the paper;
4. After the printer stop, click the “Check Status” button to display the calibration result.
5. The picture below the Label calibration curve of the label paper is the basis for label positioning;
6. The picture below the RFID signal range diagram is a signal distribution diagram of a single RFID tag. Under normal circumstances, the tag read/write area height is more than 5mm, and the position is close to the middle of the tag is better.

Software environment:
WinXP,Win7,Win8.1,Win10,Win11

If you have any other problems, please contact us with email.

ZMIN Technologies
Web:www.zmin.com.cn/en/
Email:support@zmin.com.cn
